
**Live Plug Connector**

**Technical Specifications** **V2.5**

****

**Worldwide Locations**

|  |  |
| --- | --- |
| **World Headquarters, United States of America** | **Central/South America and the Caribbean** |
| **Vivax-Metrotech Corporation**  3251 Olcott Street, Santa Clara, CA 95054, USA  T/Free : 1-800-638-7682  Tel : +1-408-962-9990  Fax : +1-408-734-1799  Website : [*www.vivax-metrotech.com*](http://www.vivax-metrotech.com)  Email : [*SalesUSA@vxmt.com*](mailto:SalesUSA@vxmt.com) | **Ventas para América Latina**  3251 Olcott Street, Santa Clara, CA 95054, USA  T/Free : 1-800-446-3392  Tel : +1-408-734-1400  Fax : +1-408-743-5597  Website : [*www.vivax-metrotech.com*](http://www.vivax-metrotech.com)  Email : *LatinSales@vxmt.com* |
| **Canada** | **United Kingdom** |
| **Vivax Canada, Inc.**  41 Courtland Ave Unit 8,Vaughan, ON L4K 3T3, Canada  Tel : +1-289-846-3010  Fax : +1-905-752-0214  Website : *www.vivax-metrotech.com*  Email : *SalesCA@vxmt.com* | **Vivax-Metrotech Ltd.**  Unit 1, B/C Polden Business Centre, Bristol Road, Bridgwater, Somerset, TA6 4AW, UK  Tel : +44(0)1793 822679  Website : [*www.vivax-metrotech.com*](http://www.vivax-metrotech.com)  Email : *SalesUK@vxmt.com* |
| **France** | **Germany** |
| **Vivax-Metrotech SAS**  Technoparc ‐ 1 allée du Moulin Berger,69130 Ecully, France  Tel : +33(0)4 72 53 03 03  Fax : +33(0)4 72 53 03 13  Website : *www.vivax-metrotech.fr*  Email : *SalesFR@vxmt.com* | **Metrotech Vertriebs GmbH**  Am steinernen Kreuz 10a  D-96110 Schesslitz  Tel : +49 954 277 227 43  Website : *www.vivax-metrotech.de*  Email : *SalesEU@vxmt.com* |

1. **Typical Applications**

|  |  |
| --- | --- |
| **Item** | **Parameter** |
| **Description** | Live Plug Connector (LPC Separation Filter) |
| **Uses** | To apply the transmitter signal to target lines carrying up to 240V AC |

1. **Characteristics**

|  |  |
| --- | --- |
| **Item** | **Parameter** |
| **Construction** | High impact ABS injection molded housing |
| **Weight** | 0.8lbs *(0.36kg)* |
| **Dimension** | 2.5-inch (Dia.) x 6.2-inch (L) *(64mm x 156.4mm*) |
| **Temperature Range** | Operating: -4ºF to 122ºF (*-20ºC to 50ºC*)  Storage: -40ºF to 140ºF (*-40ºC to 60ºC*) |
| **What's in the Box** | * Live Plug Connector * 3-Pin Power cord (per region) * Quick Guide |
| **External Connectors** | 1 x XLR 3-Pin plug connects to the transmitter  1 x 3-Pin AC Plug for up to 240V AC |
| **Compatible Transmitters** | Loc3 series, Loc series, VM series, vScan |

1. **Operational**

|  |  |
| --- | --- |
| **Item** | **Parameter** |
| **Controls** | Rotary knob – phase switching |
| **Operating Frequencies** | 8 kHz, 33 kHz, 65 kHz |

1. **Shipping and Packaging**

|  |  |
| --- | --- |
| **Item** | **Parameter** |
| **Shipping Weight** | 1.4lbs *(0.64kg)* |
| **Shipping Dimensions** | 8.7-inch(L) x 5-inch(W) x 2.7-inch(H) *(222mm x 127mm x 68mm)* |

1. **Warranty**

|  |  |
| --- | --- |
| **Item** | **Parameter** |
| **Warranty** | 12 months |

All products are designed and manufactured per ISO 9001:2015.

Disclaimer: Product and accessory specification and availability information are subject to change without prior notice.